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D3K Micropump 

Range for Gases

TCS MICROPUMPS: D3K 
(Patents Pending, Quality Assured ISO 9001, RoHS compliant, IP45 protection rating)
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Introduction
The TCS D3k Micropumps are high-quality pumps designed for use with gases only. They are highly efficient, small and lightweight. The solid construction and wide temperature tolerance, enable them to perform reliably even in hostile environments. Your Micropump can be quickly and easily installed into the smallest spaces, in a vast range of laboratory, prototype and production equipment.

Electrical Connection
Supply

Voltage:
2.0v to 6.0v DC 
Connection

Positive +:
Red Lead

Negative -:
Black Lead

Your Micropump can be connected to batteries, a DC power source of up to 6.0V or a TCS power supply TCS-600 (see accessories page on website).

Pumping rate can be adjusted by varying input voltages between 2.0v and 6.0vdc 


Materials


Housing 
PC/ABS
Seals
Nitrile
Fixings
Stainless Steel 316
Internal fixings
Nylon

Hose Connections

2.4mm (3/32”) bore flexible tubing
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Notes on Operation

For maximum flow the pump heads should be connected in parallel. Connect both the inlet ports together and both the outlet ports together.
For maximum pressure connect the pump heads in series. Connect one pump heads inlet to the second heads outlet.  The remaining ports are then become the main inlet and outlet ports for the pump.
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